***SWH TOOLKIT DOCUMENT #2B***

Your City logo here

**Eligibility Checklist for Expedited**

**Solar Pool Heating Permitting**

**for One- and Two-Family Dwellings**

GENERAL REQUIREMENTS

|  |  |  |  |
| --- | --- | --- | --- |
| A. | System size is 30 kWth (462 square feet of collector) or less | Y | N |
| B. | The solar array is roof-mounted on one- or two-family dwelling or accessory structure | Y | N |
| C. | The solar collector arrays will not exceed the maximum legal building height | Y | N |
| D. | Solar collectors are certified by an accredited listing agency | Y | N |
| E. | Building Permit application is completed and attached | Y | N |
| F. | Heat transfer fluid is either water or a nontoxic fluid | Y | N |

|  |  |
| --- | --- |
| PLUMBING REQUIREMENTS |  |
| A. Adequate extreme temperature protection is provided (if applicable)B. Standard one-line plumbing diagram is provided with components showing solarinterface with existing plumbing | YY | NN |
| STRUCTURAL REQUIREMENTS |  |  |
| A. A completed Structural Criteria and supporting documentation is attached (as required) | Y | N |

*Notes:*

*These criteria are intended for streamlined solar permitting process.*

*1. If any items are checked NO, revise design to fit within Eligibility Checklist, otherwise permit application*

*may go through standard process.*